(footprint "RotaryEncoder_EC11B-Horizontal-Dual" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a81155bc-9d15-4654-b3f7-18a5b2be92c0)
  )
  (fp_text value "RotaryEncoder_EC11B-Horizontal-Dual" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 44d178af-e812-4821-80f4-c8b9d7b1ea80)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 51781a4b-d14b-4cdd-b632-351665534537)
  )
  (fp_rect (start -7.92 -3.15) (end 7.92 4.2)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 2ffc9ca1-f48e-4a36-86a6-80c8d73a9839))
  (pad "" thru_hole oval (at -5.8 0.3125) (size 2.4 3.825) (drill oval 1.9 3.425) (layers "*.Cu" "*.Mask") (tstamp ac5ea4e4-3421-491c-a9df-956d10662f0b))
  (pad "" thru_hole oval (at 5.8 0.3125) (size 2.4 3.825) (drill oval 1.9 3.425) (layers "*.Cu" "*.Mask") (tstamp d5f26e8d-8187-4161-af4f-31b9e71e4e8e))
  (pad "A" thru_hole circle (at -2.5 1.25) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 74bc93e0-5afe-41b8-9f35-e63686e04108))
  (pad "B" thru_hole circle (at 2.5 1.25) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 52bbba4b-7e2d-466a-b42b-12f6ab33f5c2))
  (pad "C" thru_hole circle (at 0 1.25) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 2c45b371-9b8e-42c8-bdd5-4f6d474df10e))
  (pad "S1" thru_hole circle (at -2.5 -1.25) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 91515bce-ae49-46f6-a6d4-251d8dfb69f6))
  (pad "S2" thru_hole circle (at 2.5 -1.25) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp fd129759-59b7-4afc-9202-6c07ff008728))
  (model "/Users/danny/syncproj/kicad-libs/footprints/Keebio-Parts.pretty/3dmodels/EC11B-SW-Horiz-15K-blue.step"
    (offset (xyz 0 -5 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
