(footprint "Visaton BF32" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 732a89e5-8eff-4f92-80d9-13a3ed9e3e6f)
  )
  (fp_text value "Visaton BF32" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1b25a2a9-ac27-427c-bcff-a9d1bc2aae78)
  )
  (fp_text user "+" (at 6.88 -5.97 unlocked) (layer "F.SilkS")
      (effects (font (size 2 2) (thickness 0.2)) (justify left bottom))
    (tstamp 4592b0b5-cdea-48d8-8021-b8d26f1791bc)
  )
  (fp_rect (start -16 -16) (end 16 16)
    (stroke (width 0.2) (type default)) (fill none) (layer "F.SilkS") (tstamp 875c8916-9b34-4203-9d61-e890bc6e4b2a))
  (fp_circle (center -12.25 -12.25) (end -11.25 -12.25)
    (stroke (width 0.2) (type default)) (fill none) (layer "F.SilkS") (tstamp 0eb30be8-3b04-48d3-8f65-d5443900377a))
  (fp_circle (center -12.25 12.25) (end -11.25 12.25)
    (stroke (width 0.2) (type default)) (fill none) (layer "F.SilkS") (tstamp ac620a31-b5fd-4541-948c-c72ad00207ba))
  (fp_circle (center 0 0) (end 9.057974 0)
    (stroke (width 0.4) (type default)) (fill none) (layer "F.SilkS") (tstamp 775af1fb-4a0f-4a72-bf2c-1931cf6c585f))
  (fp_circle (center 0 0) (end 13.5 0)
    (stroke (width 0.2) (type default)) (fill none) (layer "F.SilkS") (tstamp 96c30893-161b-4635-9c6c-b93df3ee6d01))
  (fp_circle (center 12.25 -12.25) (end 13.25 -12.25)
    (stroke (width 0.2) (type default)) (fill none) (layer "F.SilkS") (tstamp 16b9f173-ea1b-42a0-a7d9-d15c4d627723))
  (fp_circle (center 12.25 12.25) (end 13.25 12.25)
    (stroke (width 0.2) (type default)) (fill none) (layer "F.SilkS") (tstamp 2f455677-6cd8-4775-80b9-86cfc0901351))
  (fp_circle (center 12.7 -12.7) (end 12.7 -12.7)
    (stroke (width 0.2) (type default)) (fill none) (layer "F.SilkS") (tstamp 5f8cba10-4058-4aae-9a8b-35e1e2cedde3))
  (pad "1" smd circle (at 12 -7) (size 5 5) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2dfd9487-615a-4187-8e11-9f2b428c65d7))
  (pad "2" smd circle (at -12 7) (size 5 5) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp aafe1f41-d452-49a8-bbc0-eb0651781737))
)
