(footprint "Potentiometer_Alps_RK09K_Single_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "111009J 1110AK4 11100DN 1110AAR 1110077 1110A0J 110AMJ 1110B26 D1110C1A Potentiometer, horizontal, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
  (tags "Potentiometer horizontal Alps RK09K Single Snapin")
  (property "Sheetfile" "BJ-Keyer.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Potentiometer")
  (property "ki_keywords" "resistor variable")
  (attr through_hole)
  (fp_text reference "RV1" (at 0 11.05 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e4cc8574-bded-48aa-84d3-0178444cd569)
  )
  (fp_text value "10k Log" (at 0 -6.05 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e882e795-fa44-43d7-8047-0cc45643b897)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 12c9f2b8-a04d-424e-a822-18ca7004de0d)
  )
  (fp_line (start -11.72 5.62) (end -11.72 -0.62)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bbd0b359-b5fb-4f7f-9158-d402c81a1f3a))
  (fp_line (start -4.32 -0.62) (end -11.72 -0.62)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5765c45c-0c17-48b8-9624-a3d2a3fcf93f))
  (fp_line (start -4.32 5.62) (end -11.72 5.62)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 93c9faed-ffcb-4960-b38c-3e4019acc5a2))
  (fp_line (start -4.32 5.87) (end -4.32 -0.87)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e5eb9bbe-0d51-4698-af0e-3460a93e5e9b))
  (fp_line (start -3.52 -0.87) (end -4.32 -0.87)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 59491d16-a220-445d-9376-157ad5a02b2e))
  (fp_line (start -3.52 5.87) (end -4.32 5.87)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 975ec121-f843-4fea-8c15-845408158a0c))
  (fp_line (start -3.52 7.521) (end -3.52 -2.52)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2489d901-1968-4035-b8ee-4f517f7efca1))
  (fp_line (start -2.75 -2.52) (end -3.52 -2.52)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cc17d6b0-0596-4e90-9acf-20ab717c572c))
  (fp_line (start -2.75 7.521) (end -3.52 7.521)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 49dc3740-d571-48ff-be0e-c495d465be0d))
  (fp_line (start -1.25 -2.52) (end 1 -2.52)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 14399f7e-9ecc-40d7-aaf3-2516b726635a))
  (fp_line (start 1 7.521) (end -1.25 7.521)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 22449569-c36e-4345-b0e8-44f8f1427b68))
  (fp_line (start 3.52 4.944) (end 3.52 0.055)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c91dce62-6f76-480c-a4b8-056d1d1efc34))
  (fp_rect (start -2.75 -2.52) (end -1.25 -1.85)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 19642d3a-d16e-483c-9ac6-f8fa3cb5ff89))
  (fp_rect (start -2.75 6.85) (end -1.25 7.521)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp ed9f8b1e-312d-4af6-a940-5153f94ad4ce))
  (fp_line (start -11.85 -5.1) (end -11.85 10.05)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c924e16b-daf3-4290-8180-b0f779f80e62))
  (fp_line (start -11.85 10.05) (end 5.85 10.05)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8c7a6a18-5e98-4099-97d8-de06406847e6))
  (fp_line (start 5.85 -5.1) (end -11.85 -5.1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4d64b4bf-86ae-48ea-b29f-c35b1f1f608f))
  (fp_line (start 5.85 10.05) (end 5.85 -5.1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b5a20cf1-4127-4f2c-8ae7-66c2a165f6f8))
  (fp_line (start -11.6 -0.5) (end -11.6 5.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 363a6ed9-902e-4234-9f46-4a0b2095ff2e))
  (fp_line (start -11.6 5.5) (end -4.2 5.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c4c6506a-9c8d-4432-b0db-46897327a3c4))
  (fp_line (start -4.2 -0.75) (end -4.2 5.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 13dcdc1a-d511-477c-a63c-38542951b588))
  (fp_line (start -4.2 -0.5) (end -11.6 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 92f327d4-cd98-4503-a389-7a4f52acfcec))
  (fp_line (start -4.2 5.75) (end -3.4 5.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 52ed04ab-73f9-4876-adaa-702c01259833))
  (fp_line (start -3.4 -2.4) (end -3.4 7.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3e9dfdd0-5df6-4254-aa17-fd91cc5ad003))
  (fp_line (start -3.4 -0.75) (end -4.2 -0.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 402f1a41-eee0-4bdc-8423-2891ea27380b))
  (fp_line (start -3.4 7.4) (end 3.4 7.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5d4c92aa-b120-4a9b-90d3-c2584854bfe9))
  (fp_line (start 3.4 -2.4) (end -3.4 -2.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a7d63592-e539-4f50-aaa6-ac0bd152d8cb))
  (fp_line (start 3.4 7.4) (end 3.4 -2.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1763b6b8-3496-4ce8-8847-3110a5cfa42a))
  (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask") (tstamp e016e63e-f13e-46b4-821b-9ed0eb17f694))
  (pad "2" thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask") (tstamp de443ccc-b178-4601-85d1-e7105def48d4))
  (pad "3" thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask") (tstamp ad1e4287-fcb3-48e6-b378-109d709920bb))
  (pad "MP" thru_hole roundrect (at 3.3 -2.5 180) (size 4 3) (drill oval 2.1 1.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp bf62716b-d0bd-4f6c-97ae-d8ae300cffcf))
  (pad "MP" thru_hole roundrect (at 3.3 7.5 180) (size 4 3) (drill oval 2.1 1.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp eb06b2f5-2fb2-40e4-8491-830a9fea7e5d))
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 019054cf-d79c-4a5d-b30c-3b521f62dfee) (name "Copper Keep Out") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.75 -2.5)
        (xy -1.25 -2.5)
        (xy -1.25 -1.85)
        (xy -2.75 -1.85)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 2c2e9408-cc5c-4439-bfbc-ada0a134c272) (name "Copper Keep Out") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.75 6.85)
        (xy -1.25 6.85)
        (xy -1.25 7.5)
        (xy -2.75 7.5)
      )
    )
  )
  (model "${KIPRJMOD}/3D-Models/RK09K1110-K20.step"
    (offset (xyz -3 -2.5 6.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -180 -180 -90))
  )
)
