(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "TS04-66-85-BK-160-SMT" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "S1" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "~" (at 0.635 5.969 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "SW_TS04-66-85-BK-160-SMT" (at -5.08 -0.254 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "PARTREV" "1.0" (at -1.524 -2.794 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER" "CUI Devices" (at -4.953 1.143 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (at -5.08 -1.524 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "TS04-66-85-BK-160-SMT_0_0"
      (circle (center 0 -1.905) (radius 0.635)
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -2.54)
          (xy 0 -3.683)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy 0 2.54)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.508 -1.27)
          (xy 2.159 1.651)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (circle (center 0 1.905) (radius 0.635)
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
    )
    (symbol "TS04-66-85-BK-160-SMT_1_0"
      (polyline
        (pts
          (xy 1.27 0.127)
          (xy 2.159 -0.381)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.413 0.127)
          (xy 1.905 -0.889)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "~" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -2.54 -3.81 0) (length 2.54)
        (name "~" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 2.54 3.81 180) (length 2.54)
        (name "3" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 2.54 -3.81 180) (length 2.54)
        (name "~" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
