(footprint "mouse-bite-2.54mm-slot" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "mouse-bite-2.54mm-slot" (at 0 -2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.2)))
    (tstamp ea9348cb-d2b8-430b-8970-c76c047647d2)
  )
  (fp_text value "VAL**" (at 0 2.1) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.2)))
    (tstamp b5a8b546-7d50-4b70-b2a0-c9db74af9a25)
  )
  (fp_arc (start -2.33 -1.27) (mid -1.06 0) (end -2.33 1.27)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 024f6a84-5de5-448b-a302-b3b784172b51))
  (fp_arc (start 2.33 1.27) (mid 1.06 0) (end 2.33 -1.27)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 1ec39a54-a004-4edd-8094-d3adaf8a0a59))
  (fp_circle (center -2.33 0) (end -2.27 0)
    (stroke (width 0.05) (type solid)) (fill none) (layer "Dwgs.User") (tstamp 34faa274-14e5-4957-a85c-36695c6e84a8))
  (fp_circle (center 2.33 0) (end 2.33 -0.06)
    (stroke (width 0.05) (type solid)) (fill none) (layer "Dwgs.User") (tstamp dd1a5c0a-4e28-4f12-949a-87c78078dff2))
  (fp_line (start -2.33 0) (end -2.33 0)
    (stroke (width 2.54) (type solid)) (layer "Eco1.User") (tstamp e4c480c2-bd48-4885-9d06-a3eb7448856b))
  (fp_line (start 2.33 0) (end 2.33 0)
    (stroke (width 2.54) (type solid)) (layer "Eco1.User") (tstamp 0550e973-4b4d-4a99-a61a-e7df9d9754e6))
  (pad "" np_thru_hole circle (at -0.8 -1.1) (size 0.5 0.5) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp da7ee3d0-0bcf-4f65-b1d6-100b1a843def))
  (pad "" np_thru_hole circle (at -0.8 1.1) (size 0.5 0.5) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp b8327fd3-d3f4-4ba6-8391-475bb813a4e7))
  (pad "" np_thru_hole circle (at 0 -1.1) (size 0.5 0.5) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp ab6abab8-ed86-4251-b4b4-e6d3a1eada0f))
  (pad "" np_thru_hole circle (at 0 1.1) (size 0.5 0.5) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp de17c958-8137-4dab-b725-c92348dd28f6))
  (pad "" np_thru_hole circle (at 0.8 -1.1) (size 0.5 0.5) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp 04d67fa3-c3e9-4d67-ad88-47f118279eb3))
  (pad "" np_thru_hole circle (at 0.8 1.1) (size 0.5 0.5) (drill 0.5) (layers "*.Cu" "*.Mask") (tstamp e888cbea-f84c-4df1-9066-d8ee539e6c18))
)
