
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "SMS-2008MS-R" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at -1.27 6.35 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "SMS-2008MS-R" (id 1) (at -1.27 -8.255 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "SPKR_SMS-2008MS-R" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "5/14/2020" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "4.80 mm" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Pui Audio" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "SMS-2008MS-R_0_0"
      (polyline
        (pts (xy -3.175 1.905) (xy -3.175 -1.905)) (stroke (width 0.254))
      )
      (polyline
        (pts (xy -3.175 -1.905) (xy -2.54 -1.905)) (stroke (width 0.254))
      )
      (polyline
        (pts (xy 0.0 -1.905) (xy 0.0 1.905)) (stroke (width 0.254))
      )
      (polyline
        (pts (xy -3.175 1.905) (xy -2.54 1.905)) (stroke (width 0.254))
      )
      (polyline
        (pts (xy 0.0 -1.905) (xy 2.54 -5.08)) (stroke (width 0.254))
      )
      (polyline
        (pts (xy 2.54 -5.08) (xy 2.54 5.08)) (stroke (width 0.254))
      )
      (polyline
        (pts (xy 0.0 1.905) (xy 2.54 5.08)) (stroke (width 0.254))
      )
      (polyline
        (pts (xy -2.54 -2.54) (xy -2.54 -1.905)) (stroke (width 0.1524))
      )
      (polyline
        (pts (xy -2.54 -1.905) (xy 0.0 -1.905)) (stroke (width 0.254))
      )
      (polyline
        (pts (xy -2.54 2.54) (xy -2.54 1.905)) (stroke (width 0.1524))
      )
      (polyline
        (pts (xy -2.54 1.905) (xy 0.0 1.905)) (stroke (width 0.254))
      )
      (text "+" (at -5.08 2.54 0)
        (effects (font (size 1.778 1.778)) (justify bottom left))
      )
      (text "-" (at -5.08 -5.08 0)
        (effects (font (size 1.778 1.778)) (justify bottom left))
      )
      (pin passive line (at -2.54 -5.08 90.0) (length 2.54)
        (name "~"
          (effects (font (size 1.016 1.016)))
        )
        (number "LEAD-"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -2.54 5.08 270.0) (length 2.54)
        (name "~"
          (effects (font (size 1.016 1.016)))
        )
        (number "LEAD+"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)