(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "FT230XS" (in_bom yes) (on_board yes)
    (property "Reference" "U3" (at -6.6828 -18.4442 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "FT230XS" (at -6.6828 -15.8001 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm" (at 25.4 -15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT230X.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "FTDI USB UART interface converter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Full Speed USB to Basic UART, SSOP-16" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP*3.9x4.9*P0.635mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "FT230XS_0_1"
      (rectangle (start -13.97 13.97) (end 13.97 -13.97)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "FT230XS_1_1"
      (pin output line (at 17.78 10.16 180) (length 3.81)
        (name "TXD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -17.78 10.16 0) (length 3.81)
        (name "3V3OUT" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 -5.08 0) (length 3.81)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 17.78 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -17.78 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -5.08 180) (length 3.81)
        (name "CBUS1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -2.54 180) (length 3.81)
        (name "CBUS0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -10.16 180) (length 3.81)
        (name "CBUS3" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 17.78 5.08 180) (length 3.81)
        (name "~{RTS}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 17.78 270) (length 3.81)
        (name "VCCIO" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 17.78 7.62 180) (length 3.81)
        (name "RXD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -17.78 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 17.78 2.54 180) (length 3.81)
        (name "~{CTS}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -7.62 180) (length 3.81)
        (name "CBUS2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 0 0) (length 3.81)
        (name "USBDP" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 2.54 0) (length 3.81)
        (name "USBDM" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
