(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "UJ2-MIBH2-4-SMT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at -5.08 10.1854 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "UJ2-MIBH2-4-SMT" (at -5.08 -22.8854 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "CUI_UJ2-MIBH2-4-SMT" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER" "CUI INC" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "PART_REV" "1.0" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "STANDARD" "MANUFACTURER RECOMMENDATIONS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "UJ2-MIBH2-4-SMT_0_0"
      (rectangle (start -5.08 -20.32) (end 5.08 10.16)
        (stroke (width 0.254) (type solid))
        (fill (type background))
      )
      (pin passive line (at 10.16 7.62 180) (length 5.08)
        (name "1" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 10.16 5.08 180) (length 5.08)
        (name "2" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 10.16 2.54 180) (length 5.08)
        (name "3" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 10.16 0 180) (length 5.08)
        (name "4" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 10.16 -2.54 180) (length 5.08)
        (name "5" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 10.16 -7.62 180) (length 5.08)
        (name "SHIELD" (effects (font (size 1.016 1.016))))
        (number "SH1" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 10.16 -10.16 180) (length 5.08)
        (name "SHIELD__1" (effects (font (size 1.016 1.016))))
        (number "SH2" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 10.16 -12.7 180) (length 5.08)
        (name "SHIELD__2" (effects (font (size 1.016 1.016))))
        (number "SH3" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 10.16 -15.24 180) (length 5.08)
        (name "SHIELD__3" (effects (font (size 1.016 1.016))))
        (number "SH4" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 10.16 -17.78 180) (length 5.08)
        (name "SHIELD__4" (effects (font (size 1.016 1.016))))
        (number "SH5" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
